{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["推荐候选人名单及申报成果"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"推荐候选人名单及申报成果","index":0,"n_rows":23,"n_cols":16,"rows_kept":23,"merged":[[0,0,0,9],[1,6,1,7],[2,0,11,0],[2,1,11,1],[2,1,11,1],[2,2,11,2],[2,3,11,3],[2,4,11,4],[2,5,11,5],[12,0,12,9],[13,6,13,7],[14,0,22,0],[14,1,22,1],[14,1,22,1],[14,2,22,2],[14,3,22,3],[14,4,22,4],[14,5,22,5]],"flags":["formulas_cached_only"]}
["2018年“唐立新奖学金”推荐候选人及申报成果(DNL17)"]
["序号","姓名","入学年份","攻读类别","专业","指导教师","论文(成果)名称",null,"作者署名顺序/作者总数","发表刊物[名称,doi]"]
[1,"鲁文静",2014,"硕博","化学工程","李先锋",1,"Porous membranes in secondary battery technologies","1/6","CHEMICAL SOCIETY REVIEWS,10.1039/c6cs00823b"]
[{"$nulls":6},2,"High-performance porous uncharged membranes for vanadium flow battery applications created by tuning cohesive and swelling forces","1/6","Energy & Environmental Science,10.1039/c6ee01371f"]
[{"$nulls":6},3,"Solvent-Induced Rearrangement of Ion-Transport Channels: A Way to Create Advanced Porous Membranes for Vanadium Flow Batteries","1/6","ADVANCED FUNCTIONAL MATERIALS,10.1002/adfm.201604587",{"$nulls":5}," "]
[{"$nulls":6},4,"The next generation vanadium flow batteries with high power density – a perspective","1/3","PHYSICAL CHEMISTRY CHEMICAL PHYSICS,10.1039/c7cp07456e"]
[{"$nulls":6},5,"Advanced porous PBI membranes with tunable performance induced by the polymer-solvent interaction for flow battery application","1/6","Energy Storage Materials,http://dx.doi.org/10.1016/j.ensm.2017.08.004"]
[{"$nulls":6},6,"Advanced charged porous membranes with ﬂexible internal crosslinking structures for vanadium ﬂow batteries","2/6","Journal of Materials Chemistry A,10.1039/c7ta00117g"]
[{"$nulls":6},7,"The porous membrane with tunable performance for vanadium flow battery: The effect of charge","3/5","JOURNAL OF POWER SOURCES,10.1016/j.jpowsour.2016.12.058"]
[{"$nulls":6},8,"一种液流电池用聚合物多孔离子传导膜的溶剂处理方法","3/5","发明专利,201610443530.2"]
[{"$nulls":6},9,"一种溶剂处理过程中液流电池用聚合物多孔离子传导膜的溶剂筛选办法","3/6","发明专利,201710940848.6"]
[{"$nulls":6},10,"一种液流电池用离子传导膜及其制备和应用","5/6","发明专利,201710940705.5"]
["2018年“唐立新奖学金”推荐候选人及申报成果(1101组)"]
["序号","姓名","入学年份","攻读类别","专业","指导教师","论文(成果)名称",null,"作者署名顺序/作者总数","发表刊物[名称,doi]"]
[2,"杨斌",2014,"直博","物理化学","何国钟韩克利",1,"Ultra-Sensitive and Fast All-Inorganic Perovskite based Photodetector via Fast Carrier Diffusion","1/8","ADVANCED MATERIALS,10.1002/(adma.201703758R1)"]
[{"$nulls":6},2,"Lead-Free, Air-Stable All-Inorganic Cesium Bismuth Halide Perovskite Nanocrystals","1/10","ANGEWANDTE CHEMIE-INTERNATIONAL EDITION,10.1002/anie.201704739R1"]
[{"$nulls":6},3,"Lead-Free Silver-Bismuth Halide Double Perovskite Nanocrystals","1/9","ANGEWANDTE CHEMIE-INTERNATIONAL EDITION,DOI: 10.1002/anie.201800660"]
[{"$nulls":6},4,"Constructing Sensitive and Fast Lead-Free Single Crystalline Perovskite Photodetectors","1/8","Journal of Physical Chemistry Letters,DOI: 10.1021/acs.jpclett.8b01116"]
[{"$nulls":6},5,"Low Threshold Two-Photon-Pumped Amplified Spontaneous Emission in CH3NH3PbBr3 Microdisks","1/8","ACS Applied Materials & Interfaces,10.1021/acsami.6b04246"]
[{"$nulls":6},6,"Perovskite CH3NH3PbI3−xBrx Single Crystals with Charge-Carrier Lifetimes Exceeding 260 μs(非第一单位)","2/11","ACS Applied Materials & Interfaces,10.1021/acsami.7b01696"]
[{"$nulls":6},7,"Extra long electron–hole diffusion lengths in CH3NH3PbI3\u0002xClx perovskite single crystals(非第一单位)","2/5","Journal of Materials Chemistry C,DOI: 10.1039/c7tc02802d"]
[{"$nulls":6},8,"Formamidinium Lead Bromide (FAPbBr3) Perovskite Microcrystals for Sensitive and Fast Photodetectors(非第一单位)","2/7","Nano-Micro Letters,doi.org/10.1007/s40820-018-0196-2"]
[{"$nulls":6},9,"Photostability of the Oleic Acid-Encapsulated Water-Soluble CdxSeyZn1−xS1−y Gradient Core−Shell Quantum Dots(非第一单位)","2/6","acs omega,10.1021/acsomega.7b00316"]